Note! Complete this sheet after servicing a Varec 2500 ATG in conjunction with an API 653 bulk storage tank inspection, repair, alteration, and reconstruction.

Note! One Detailed Tank Inspection Report (FRM056) per tank must be attached to final inspector report.

|  |  |  |  |
| --- | --- | --- | --- |
| **Internal Tank Inspection** | **Yes** | **No** | **N/A** |
| Tape replaced?  |  |  |  |
| Guide wires taut? |  |  |  |
| Tape clamp properly installed? |  |  |  |
| Tape not twisted from the float to the roof? |  |  |  |
| Float installed on the guide wires?  |  |  |  |
| Float moves up and down freely?  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **2500 ATG Inspection** | **Yes** | **No** | **N/A** |
| Counter assembly (21) replaced?  |  |  |  |
| Counter (21) adjusted properly? |  |  |  |
| Counter shaft (11) turns freely? |  |  |  |
| Dial assembly (7) replaced? |  |  |  |
| Dial assembly (7) set for 16th or 10th inch?  |  |  |  |
| The gauge needs to be calibrated with product in the tank  |  |  |  |

Inspected By: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_\_\_\_\_\_

*This document can be downloaded from www.varec.com*